Southern Sweepers & Scrubbers

# Contact us: 877 -377-7552 I southernsweepers.com

830- II Operator Checklist

Pre-Operation Checklist

D Check brake fluid level.

D Check windshield fluid level.

D Check right front tire pressure.

D Check air intake duct screen.

D Check radiator overflow reservoir.

D Check engine oil level.

D Check hydraulic fluid level using site gauge.

D Check fuel water trap.

D Check right hand conveyor bearing housing backlash bolt.

D Check right -hand dry dust control skirt for wear.

D Check right -hand dust control spray nozzles adjustments/ condition.

0 Check right -sidebrush for debris and wear.

D Check center debris skirt for wear.

0 Inspect conveyor paddles.

D Inspect hopper/conveyor seal for wear

D Inspect main brush for wear, banding materials, debris.

0 Inspect conveyor lips & skirts.

D Inspect main brush compartment right-hand skirts/skids.

D Check right rear tire pressure.

D Inspect hopper door seal.

D Inspect vacuum wand hose.

0 Inspect hopper dust filter condition

D Check left rear tire pressure.

0 Inspect main brush compartment left-handskir ts/skids.

D Check left-hand conveyor bearing housing backlash bolt.

D Check radiator fluid level.

D Check radiator & hydraulic oil cooler fins for blockage.

D Check wet dust control water fill hose.

D Check wet dust water tank fluid level.

D Inspect left-hand brush dry dust control skirt for wear.

D Check left-hand wet dust control spray nozzle adjustments.

D Inspect left-side brush for debris and wear.

D Check left front tire pressure.

D Check left-side mirrors.

D Check wiper blades.

0 Check Vario brush for debris and wear.

D Check Vario brush dust control nozzle adjustment.

D Check right -side mirrors record hour meter reading .

List any problems that occurred during operation:

Operator: Date:

Supervisor: Date: