Southern Sweepers & Scrubbers

[www.southernsweepers.com](http://southern-sweepers.com) | 877-377-7552

S20 Daily Operator Checklist

Pre-Operation Checklist

* Check the condition of the main brush. (For maximum brush life and best performance, remove any string, banding, plastic wrap, or other debris wrapped around the brush and rotate the main brush end to end, after every 50 hrs of operations.)
* Check the main brush compartment right handed skirt for damage and wear.
* Check the side sweeping brush for damage and wear. Remove any string, banding, plastic wrap, or other debris wrapped around the brush.
* Check the engine air filter indicator.
* Check the engine oil level
* Confirm the cooling fan screen and radiator fins are clean.
* Check the hydraulic fluid level.
* Check for leaks and rubbing hoses or wires.
* Check the highlights, taillights and the safety lights.
* Check the steering and breaks for proper operation
* Raise the hopper, set the safety leg and check the hopper skirt & brush compartment skirt for wear or damage.
* Check the service records to determine maintenance requirements.

List below any problems that occurred during operation:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Operator: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

Supervisor: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_