Southern Sweepers & Scrubbers

Contact us: 877-377-7552 | [southernsweepers.com](http://southern-sweepers.com)

8410 Daily Operator Checklist

Pre-operation Checklist

* Check under the machine for leaks (fuel, oil, coolant, scrubbing solution).Check the battery fluid and charge level.
* Check the engine air filter indicator.
* Check the engine oil level.
* Check fuel level.
* Check the brakes and steering for proper operation.
* Check the rear squeegee for wear and proper deflection. Check the side squeegees for wear.
* Check for wire, string, or twine wrapped around the sweeping and scrub brushes.
* Check the vacuum hoses for debris or obstructions.
* ES machines. Check that the ES filter and solution outlet filter is clean.
* Check for loose fittings, or wires.
* Check the condition of the v--belt.
* Check the hydraulic oil level.
* Check the cooling system level.
* ES machines. Check detergent level in the detergent tank, fill as required.
* FAST Scrubbing: Check the FaST PAK concentrate agent level, replace carton as needed. See the INSTALLING THE FaST PAK AGENT section of the manual.
* FAST Scrubbing: Check that all conventional cleaning agents/restorers are drained and rinsed from the solution tank.
* FAST Scrubbing: Check that the solution tank is filled with clear cool water only.

Post-Operation Checklist

* Check the brushes adjustment. See TO CHECK AND ADJUST MAIN BRUSH PATTERN and SIDE BRUSH in MAINTENANCE.
* Check for wire, string, or twine wrapped around the sweeping and scrub brushes.
* Check the brush skirts for damage, wear, and adjustments.
* Check the squeegees for wear or damage.
* Drain and clean the recovery tank.
* ES mode: Drain and clean the solution tank and clean the solution outlet filter. Clean the ES filter.
* Check the vacuum hoses for debris or obstructions.
* LPG powered machine: Check to make sure the LPG tank service valve is closed.
* Check for fuel odor that indicates a fuel leak.
* Check under the machine for leak spots (fuel, oil, coolant, scrubbing solution).
* Empty hopper and clean dust filter.
* Check the service records to determine maintenance requirements.
* FaST Scrubbing: If FaST PAK is empty after scrubbing, install a new FaST PAK or connect supply hose to the storage plug.

List below any problems that occurred during operation:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Operator: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

Supervisor: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_