Southern Sweepers & Scrubbers

Contact us: 877-377-7552 | [southernsweepers.com](http://southern-sweepers.com)

7300 Daily Operator Checklist

Pre-operation Checklist

* Check the hydraulic fluid level. (if applicable)
* Check the battery fluid and charge level.
* Check the tank cover seals for damage and wear.
* Clean the vacuum fan inlet filter.
* Check the condition of the scrubbing brushes. Remove any string, banding, plastic wrap, or other debris wrapped around them.
* Check the squeegees for damage, wear and for deflection adjustment.
* Check the vacuum hose for debris or blockage.
* ES machines; check the detergent tank level.
* Drain and clean the recovery tank.
* ES machines; drain and clean the solution tank and ES filter. Rinse level sensors.
* Check the brakes and steering for proper operation.
* Empty and clean the debris tray. (if applicable).
* Check the service records to determine maintenance requirements.
* FAST Scrubbing: Check the FaST PAK concentrate agent level, replace carton as needed.
* For FaST or ec--H2O Scrubbing: Check that the solution tank is filled with clear cool water only.

Post-Operation Checklist

* Check the hydraulic fluid level. (if applicable)
* Check the battery fluid and charge level.
* Check the tank cover seals for damage and wear.
* Clean the vacuum fan inlet filter.
* Check the condition of the scrubbing brushes. Remove any string, banding, plastic wrap, or other debris wrapped around them.
* Check the squeegees for damage, wear and for deflection adjustment.
* Check the vacuum hose for debris or blockage.
* ES machines; check the detergent tank level.
* Drain and clean the recovery tank.
* ES machines; drain and clean the solution tank and ES filter. Rinse level sensors.
* Check the brakes and steering for proper operation.
* Empty and clean the debris tray. (if applicable).
* Check the service records to determine maintenance requirements.
* FaST Scrubbing: If FaST PAK is empty after scrubbing, install a new FaST PAK or connect supply hose to the storage plug.

List below any problems that occurred during operation:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Operator: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

Supervisor: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_