Southern Sweepers & Scrubbers

[www.southernsweepers.com](http://southern-sweepers.com) | 877-377-7552

7200 Daily Operator Checklist

Pre-Operation Checklist

* Check the machine for leaks.
* Check the squeegee blades for rounded edges and cuts.
* Clean the vacuum fan in the line filter.
* Clean the ES filter.
* Check the scrub head brushes for debris, banding, plastic wrap and twine.
* Clean the debris trough. (Cylindrical Scrub Head Only)
* Inspect the recovery tank cover seals.

Post Operation Checklist

* Clean the solution and recovery tanks.
* Clean the ES filter.
* Check the battery charge levels to determine if the battery needs charging.
* Check the squeegees for damges and wear.
* Check the vacuum hoses for blockage.
* Check the scrub head and brushes for banding, plastic wrap and twine.
* Clean the debris trough. (Cylindrical Scrub Head Only)
* Check the fluid level of all battery cells and place the machine on the charger if needed.

List below any problems that occurred during operation:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Operator: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

Supervisor: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_