Southern Sweepers & Scrubbers

[www.southernsweepers.com](http://southern-sweepers.com) | 877-377-7552

S30 Daily Operator Checklist

Pre-Operation Checklist

* Check the fuel level.
* Check the condition of the main brushes. Remove any string, banding, plastic wrap, or other debris wrapped around the brushes.
* Check the main brush compartment right-hand skirt for damage and wear.
* Check the side brush. Remove any string, banding, plastic wrap, or other debris wrapped around the brushes.
* Check the condition of the side brush skirt.
* Check the hydraulic fluid level.
* Check the main brush compartment left-hand skirt for damage or wear.
* Check the engine coolant level.
* Check the engine oil level.
* Check that the radiator and hydraulic cooler fins are clean.
* Check the headlights, taillights and safety lights.
* Check the steering and breaks for proper operation.
* Check the service records to determine maintenance requirements.

List below any problems that occurred during operation:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Operator: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

Supervisor: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_